**EC6200-7 ID General Master**

Ninety Minute Program Format

7 Act - 6 Break

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Description**  (SMPTE drop frame time code is mandatory) | | **Timecode**  **In**  hh;mm;ss;ff  **(29.97)** | **Timecode In** hh:mm:ss:ff  **(25)** | **Duration**  mm;ss;ff | **Timecode Out**  hh;mm;ss;ff  **(29.97)** | **Timecode**  **Out**  hh:mm:ss:ff  **(25)** |
| **Bars & Tone** |  | **00;59;40;00** | **09:59:40:00** | **00:04:00** | **00;59;44;00** | **09:59:44:00** |
| **Black** | **Black** | **00;59;44;00** | **09:59:44:00** | **00:01:00** | **00;59;45;00** | **09:59:45:00** |
| **Slate** | **Slate(s) main + supplemental (woos, other) :05 each** | **00;59;45;00** | **09:59:45:00** | **00:10:00** | **00;59;55;00** | **09:59:55:00** |
| **Countdown** | **Countdown from :05 to :03**  **(with audible tone at each 1 second interval)** | **00;59;55;00** | **09:59:55:00** | **00:03:00** | **00;59;57;02** | **09:59:57:02** |
| **Black** | **Black** | **00;59;57;02** | **09:59:57:02** | **00:00:06** | **00;59;57;06** | **09:59:57:06** |
| **White** | **Sync Indicator**  **(two frames of white video and 1 khz tone)** | **00;59;57;06** | **09:59:57:06** | **00:00:02** | **00;59;57;08** | **09:59:57:08** |
| **Black** | **Black** | **00;59;57;08** | **09:59:57:08** | **00:02:20 (29.97)**  **00:02:15 (25)** | **01;00;00;00** | **10:00:00:00** |
| **Content Act #1** | Beginning of program/disclaimer | **01;00;00;00** | **10:00:00:00** |  |  |  |
| **Act #1 minimum length of 12:00** |  |  |  |  |  |
| BREAK #1 | Black |  |  | 00:05:00 |  |  |
| **Content Act #2** | **Act #2** |  |  |  |  |  |
| BREAK #2 | Black |  |  | 00:05:00 |  |  |
| **Content Act #3** | **Act #3** |  |  |  |  |  |
| BREAK #3 | Black |  |  | 00:05:00 |  |  |
| **Content Act #4** | **Act #4** |  |  |  |  |  |
| BREAK #4 | Black |  |  | 00:05:00 |  |  |
| **Content Act #5** | **Act #5** | Must begin no later than  01;40;35;00 and be at least 8:00 minutes long | |  |  |  |
| BREAK #5 | Black |  |  | 00:05:00 |  |  |
| **Content Act #6** | **Act #6** | Must start no earlier than  1:40;45;00 | |  |  |  |
| BREAK #6 | Black |  |  | 00:05:00 |  |  |
| **Content Act #7** | **Act #7** |  |  |  | **02;02;30;00** | **11:02:30:00** |
| **Credits** | \*See Special Note (on page 3) | **02;02;00;00** | **11:02:00:00** | 00:30:00 | **02;02;30;00** | **11:02:30:00** |
| **Black** | **Black Post Roll -** *Must end with at least 1 sec of black video and silent audio* | | | | | |

**EC6200-7 ID General Master**

Ninety Minute Program Format

7 Act - 6 Break

**PROGRAM FORMAT SPECIFICATIONS FOR 1080i 59.94/50:**

• First program video and/or audio must hit at timecode 01;00;00;00 (NTSC) / 10:00:00:00 (PAL).

• Total Content Time **62:00** *Content Time Includes: disclaimers, program tease/open, graphic titles, Acts 1-7, full-screen card credits over black, and any other elements attached to the program.*

• Breaks (:05 x 6 breaks) **00:30** • TOTAL RUNNING TIME (TRT) **62:30**

**PROGRAM FORMAT SPECIFICATIONS FOR 1080p 23.98:**

*After Discovery converts the program to 1080i 59.94 with 29.97 drop frame time code the program will match the EC 6200-7 clock.*

• First program video and/or audio must hit at time code 01:00:00:00.

• Total Content Time cannot exceed **2;02;00;00** when timecode converted to 29.97 *Content Time Includes: disclaimers, program tease/open, graphic titles, Acts 1-7, embedded credits, and any other elements attached to the program.*

• Breaks (:05 x 6 breaks)

• TOTAL RUNNING TIME (TRT) must equal **2;02;30;00** when converted to 29.97

**EDITING GUIDELINES:**

• Segments do not have to begin and end at :00 frames, ***except*** the beginning of segment 1 and the end of segment 5

• **Segment 1** begins at 01;00;00;00 (NTSC)/10:00:00:00 (PAL).

• **Segment 7** ends at 02;02;30;00 (NTSC)/11:02:30:00 (PAL).

• Act #1 should be the longest act in the program.

• No act should be shorter than 5 minutes of content time

* All segments except for the last segment should end with a 1.5 second visual dip to black, accompanied by an audio/musical ring-out.

• **See your ID Production Team for details if there are any questions regarding segment length**

**EC6200-7 ID General Master**

Ninety Minute Program Format

7 Act - 6 Break

**SNAP-IN GUIDELINES**

*\*\*Please check the contract to verify whether Snap-In Content is a required deliverable. \*\**

**Definition**

Snap-In Content are segments for the program fully produced and packaged with music, graphics and transitions to allow Discovery to create alternate or longer versions of the program. These can be created by extending an existing scene with new footage or creating new segments from program footage that does not appear in any episode of the same series. Snap-ins are needed for reasons which include, but are not limited to, network clock changes, program versioning, and international regions with different clocks.

If program is delivering cut-to-clock, instead of a seamless program, producer must provide snap-ins to bring the total content time up to at least 48:00 for a 1x60 (24:00 for a 1x30, 72:00 for a 1x90 and 94:00 for a 1x120), so other Discovery divisions and international regions can customize the program for their markets. For example, if a show delivers at 41:30, an additional 6 minutes and 30 seconds of content will need to be delivered within the snap-ins (more than 6:30 is fine but no less)

Note: much better snap-ins will be produced if a longer version of the program is created first, and then snap the extra sections out, rather than trying to create the segments as an afterthought.

**Guidelines**

• The snap-ins must be held to the same editorial standard as the main body of the program and be editorially integrated into the storyline, consist of valuable program content and must not reuse material or sequences used elsewhere in the same program or in other episodes of the same series.

• Snap-In Content must be approved by the Network AP/CP/Producer no later than the fine cut stage.

• In general, several short snap-ins should be created rather than one or two long ones (see EXCEPTION at bottom). The ideal scenario is four to six snap-ins of 30 seconds to two minutes in duration. Specific snap-in & total master length needs are outlined in the producer’s deliverables. Snap-ins cannot repeat or reprise any content that appears in either the rest of the program or in any other episode of the same series. They can be comprised of either extensions of existing scenes or short new scenes that do not appear in the cut-to-clock version.

• Short snap-ins range from 30-90 seconds, with no snap-in shorter than 30 seconds. • Snap-ins should not be provided for only one or two segments of the program. Ideally, they should be produced to snap-in to at least four different segments.

• These segments must be fully produced with complete audio stems to match the program. • Snap-ins must be fully mixed and color corrected to match the program.

• Snap-ins must be narrated by the program narrator (if needed) and have music in keeping with the main body of the program.

• If text exists within any snap-in, a separate file containing fully textless snap-ins or textless cover shots must be delivered as well.

**EC6200-7 ID General Master**

Ninety Minute Program Format

7 Act - 6 Break

• One file containing all snap-ins (and one associated textless file, if needed) must be uploaded separately from the Program Master File. Each snap-in should be slated before video begins to clearly denote the timecode where the snap-in should be added. Slates must include snap-in durations, exact time code where snap-in is to be inserted in the program and should be named or numbered, in sequence, to avoid confusion.

• Snap-in content must be provided cut-to-cut. If that means repeating some of the material in the body of the program to be able to go backwards or forwards to a clean cut, please indicate what the overall duration of the snap-in is, in addition, to the net length of the new material. • Snap-ins must be color corrected to match the program.

• Ideally, there should be no music where a snap-in is to be snapped in. If there is, it should exactly match the outgoing and incoming music in the cut-to-clock version. It should never be a different piece of music than what is laid in where the snap-in is to be placed. Please have the editor consider the music implications when creating the snap-ins and provide elements that allow the best possible product.

• Snap-ins must be transcribed as part of the full-length script.

**EXCEPTION**

• If preferred, vendor can provide one or more long, stand-alone snap-ins (2 -4 minutes) which can be cut down if needed, in addition to various, shorter snap-ins. Note these long snap-ins must still make sense if added to the program.

• Short snap-ins that total at least 3:00 in content time must be provided in all cases (regardless of the length and number of the long snap-ins, if chosen to provide).